include/hw/pci-host/q35.h@MCH_HOST_BRIDGE_EXT_TSEG_MBYTES_SIZE;
hw/pci-host/q35.c@mch_update;
hw/pci-host/q35.c@mch_reset;
hw/pci-host/q35.c@mch_update_ext_tseg_mbytes;
include/hw/pci-host/q35.h@MCH_HOST_BRIDGE_EXT_TSEG_MBYTES_QUERY;
include/hw/pci-host/q35.h@MCHPCIState;
hw/pci-host/q35.c@mch_realize;
hw/pci-host/q35.c@mch_write_config;
hw/pci-host/q35.c@mch_update_smram;
include/hw/pci-host/q35.h@MCH_HOST_BRIDGE_EXT_TSEG_MBYTES;
hw/pci-host/q35.c@q35_host_class_init;
include/hw/pci-host/q35.h@MCH_HOST_BRIDGE_EXT_TSEG_MBYTES_MAX;
